BCGBC4007A Plan building or construction work

Develop, track and revise project timeframes

Network systems or PERT charts
Activity - Building foundations 
Order these six steps in the building of footings for a residential construction from first to last.
1.     	Dig foundations
2.     	Dig stump holes
3.     	Lay bricks for the base
4.     	Order timber and concrete
5.     	Place stumps and concrete
6.     	Set out footings
When you think you have the correct answer, check your answer against the one shown below.
1.     	Set out footings
2.     	Dig foundations
3.     	Dig stump holes
4.     	Order timber and concrete
5.     	Place stumps and concrete
6.     	Lay bricks for the base

© Copyright Commonwealth of Australia 2007